AT-OP-108L

Bill of Materials

1. RAD products:

|  |  |  |
| --- | --- | --- |
|  | For 1 pair | For 2 pairs |
| RM-35/P2 (for DXC4) | 1 | 1 |
| RM-34 (for ATE-PIO-USB, ETX-204A) | 2 | 4 |
| DXC4/8 with E1 Generator program | 1 | 2 |
| ETX-204A/AC/DTAG with Ethernet Generator program | 1 | 2 |
| SF-1V/E1/WDC/4U1S/2RS | 2 | 4 |
| SFP-9G | 2 | 4 |
| PS-240/AC/DC-48 | 1 | 1 |

1. A.T.E. products:

|  |  |  |
| --- | --- | --- |
|  | For 1 pair | For 2 pairs |
| ATE-PIO-USB | 1 | 2 |
| ATE-RELAY-BOX-4 | 1 | 1 |

1. Cables:
   1. RAD cables:

|  |  |  |
| --- | --- | --- |
|  | For 1 pair | For 2 pairs |
| CBL-DB9F-DB9M-STR | 2 | 4 |
| CBL-ETH/STP/STR | 5 | 9 |
| CBL-RJ45/D9/F/6FT | 1 | 1 |

* 1. Specify cables:

|  |  |  |
| --- | --- | --- |
|  | For 1 pair | For 2 pairs |
| AT-OP108L/CBL01 | 1 | 1 |
| AT- OP108L/CBL02 | 8 | 16 |
| AT- OP108L/CBL03 | 2 | 4 |
| AT- OP108L/CBL04 | 2 | 4 |

1. Mechanic parts:

|  |  |  |
| --- | --- | --- |
|  | For 1 pair | For 2 pairs |
| Masad (width 19”) | 1 (height 32U) | 1 |
| Fixed Shelf | 1 | 1 |
| Removeable Shelf | 1 | 2 |

1. Test equipment
   1. PC’s card

|  |  |  |
| --- | --- | --- |
|  | For 1 pair | For 2 pairs |
| Ethernet card | 1 | 1 |

* 1. Movable equipment

|  |  |  |
| --- | --- | --- |
|  | For 1 pair | For 2 pairs |
| Barcode scanner | 1 | 1 |
| USB-4xRS232 | 1 | 2 |
| 8 port 10/100 Ethernet Switch | 1 | 1 |

1. PC
   1. PC
   2. Screen
   3. Keyboard
   4. Mouse
2. Miscellaneous:
   1. 5-way long power cable 230v …...…..…… 2 units
   2. Extension power cable 230v ..………..…… 1 unit
   3. Multiple power socket ..…………………… 1 unit
   4. Mouse pad …………………………....…… 1 unit
   5. Anti static surface ……………………….…. 2 units
   6. DIN rail ……………………………………. 48 cm